
Hello John,

What kind of hardware are you using ? USB-3003 ?
USB-3003 has 3 channels, ambed will work with single USB-3003.
We’re working on the USB-3000 (ThumbDV) with single channel, in this case, paring two USB-3000 is necessary.
Currently, I got stuck in PKT_RESET, no response (i.e. PKT_READY) from USB-3000 after sending PKT_RESET.
Also, there’s also a bug for multiple USB-3003 paring codes.
If I can get the USB-3000 paring working, the similar code can be used for USB-3003 paring as well.
My current codes are here:
https://github.com/yngwiechou/xlxd/tree/master/ambed
But still struggling with PKT_RESET.
Regards,
Yngwie
BU2EA

こんにちはジョン、
どのような種類のハードウェアを使用していますか？ USB-3003？
USB-3003には3つのチャンネルがあり、1つのUSB-3003で動作します。
私たちはシングルチャンネルのUSB-3000（ThumbDV）に取り組んでいます。この場合、2つのUSB-3000をペアリングする必要があります。
現在、PKT_RESETを送信した後、USB-3000からの応答（つまりPKT_READY）がなく、PKT_RESETに固執しました。
また、複数のUSB-3003ペアリングコードのバグもあります。
私がUSB-3000のペアリングを有効にすることができれば、同様のコードをUSB-3003のペアリングにも使用できます。
私の現在のコードはここにあります：
https://github.com/yngwiechou/xlxd/tree/master/ambed
しかし、まだPKT_RESETで苦労しています。

よろしく、
イングウィ
BU2E



Hi Yngwie,

I have a USB-3012 which is recognized as 4, 3-channel devices.  So 12 channels are seen.

Bob/W6KD pointed out that the ThumbDV uses the FTDI FT230XS serial-to-USB chip.  The DVSI units use the FT232R, but both use the same unified driver set.  Apparently FTDI has a Facebook page and describes the differences.

Might be useful to look there and also on the FTDI site and see if any differences might indicate different settings in the drivers.  Just a thought.

Good luck!

John
K6KD
__._,_.___
こんにちは、

私は4,3チャンネルデバイスとして認識されるUSB-3012を持っています。 だから12チャンネルが見えます。
Bob / W6KDは、ThumbDVがFTDI FT230XSシリアル-USBチップを使用していることを指摘しました。 DVSIユニットはFT232Rを使用しますが、どちらも同じ統一ドライバセットを使用します。 どうやらFTDIにはFacebookのページがあり、その違いを説明しているようです。
そことFTDIのサイトで見て、違いがドライバの異なる設定を示しているかどうかを確認するのに役立つかもしれません。 ちょっとした考え。

がんばろう！

ジョン
K6KD

Thanks John.
Initiating USB-3012 or USB-3003 is a different story from USB-3000.
I’ll need to introduce specific codes for USB-3000 / ThumbDV.
Understood that ThumbDV uses FT230XS instead of FT232R.
Thanks for the hints, I’ll take a look at the FT230X to see if there’s any necessary change required.
Here the output of my current code, ambed finds the ThumbDV correctly.
But I wasn’t able to perform a Packet Reset.
root@compass:/ambed# /ambed/ambed 10.100.1.39
Starting AMBEd
Initializing vocodecs:
Detected 2 USB-FTDI devices
ありがとうジョン。
USB-3012またはUSB-3003の起動は、USB-3000とは別の話です。
私はUSB-3000 / ThumbDVのための特定のコードを導入する必要があります。
ThumbDVはFT232Rの代わりにFT230XSを使用していることを理解しています。
ヒントをお寄せいただきありがとうございます。私はFT230Xを見て、必要な変更が必要かどうかを見ていきます。
ここで私の現在のコードambedの出力は、ThumbDVを正しく検出します。
しかし、私はパケットリセットを実行することができませんでした。
root @ compass：/ ambed＃/ ambed / ambed 10.100.1.39
AMBEdの起動
ボコーデックの初期化：
[bookmark: _GoBack]検出された2つのUSB-FTDIデバイス
Description : USB-3000	 Serial : DN27WI1V
Description : USB-3000	 Serial : DN27WI0Z
Found USB-3000 (0) S/N: DN27WI1V
Found another USB-3000 (1) DN27WI0Z
Paring USB-3000 devices
Opening USB-3000:DN27WI1V device
Using baudrate = 460800 for USB-3000
Setting baudrate = 460800
Reseting USB-3000 device
Trying soft reset for USB-3000
[DEBUG] Sending PKT_RESET w/o Parity
[DEBUG] ftStatus = 0
[DEBUG] Get 0 bytes
FTDI_read_bytes(4) failed : 0
[DEBUG] Sending PKT_RESETSOFTCFG w/o Parity
[DEBUG] ftStatus = 0
[DEBUG] Get 0 bytes
FTDI_read_bytes(4) failed : 0
reset failure

Codec interfaces initialized successfully : 0 channels availables

Initializing controller

AMBEd started and listening on 10.100.1.39
^C
root@compass:/ambed#

Regards,
Yngwie
BU2EA
