
Guys,

there is some basic difference. Bob and John are talking about using the
buit-in Linux driver (aka. kernel module ftdi_sio) I guess.
The xlxd code makes use of the closed-source driver ft2xx by FTDI.
いくつかの基本的な違いがあります。 ボブとジョンは、
buit-in Linuxドライバ（別名カーネルモジュールftdi_sio）だと思います。
xlxdコードは、FTDIによってクローズドソースドライバft2xxを使用します。
We are currently struggeling with resetting the ThumbDV correctly.
[bookmark: _GoBack]私たちは現在、ThumbDVを正しくリセットすることに苦労しています。
vy73 de Florian DF2ET

On 08/12/2017 04:37 AM, Yngwie Chou yngwie.chou@gmail.com [xlxd-star] wrote:
> Thanks John.
> 
> Initiating USB-3012 or USB-3003 is a different story from USB-3000.
> I’ll need to introduce specific codes for USB-3000 / ThumbDV.
> 
> Understood that ThumbDV uses FT230XS instead of FT232R.
> Thanks for the hints, I’ll take a look at the FT230X to see if there’s
> any necessary change required.
> 
> Here the output of my current code, ambed finds the ThumbDV correctly.
> But I wasn’t able to perform a Packet Reset.
> 
> root@compass:/ambed# /ambed/ambed 10.100.1.39
> Starting AMBEd
> 
> Initializing vocodecs:
> Detected 2 USB-FTDI devices
> 
> Description : USB-3000Serial : DN27WI1V
> Description : USB-3000Serial : DN27WI0Z
> Found USB-3000 (0) S/N: DN27WI1V
> Found another USB-3000 (1) DN27WI0Z
> Paring USB-3000 devices
> Opening USB-3000:DN27WI1V device
> Using baudrate = 460800 for USB-3000
> Setting baudrate = 460800
> Reseting USB-3000 device
> Trying soft reset for USB-3000
> [DEBUG] Sending PKT_RESET w/o Parity
> [DEBUG] ftStatus = 0
> [DEBUG] Get 0 bytes
> FTDI_read_bytes(4) failed : 0
> [DEBUG] Sending PKT_RESETSOFTCFG w/o Parity
> [DEBUG] ftStatus = 0
> [DEBUG] Get 0 bytes
> FTDI_read_bytes(4) failed : 0
> reset failure
> 
> Codec interfaces initialized successfully : 0 channels availables
> 
> Initializing controller
> 
> AMBEd started and listening on 10.100.1.39
> ^C
> root@compass:/ambed#
> 
> 
> Regards,
> Yngwie
> BU2EA
> 
>> On Aug 12, 2017, at 10:25, john_fields@yahoo.com
>> <mailto:john_fields@yahoo.com> [xlxd-star] <xlxd-star@yahoogroups.com
>> <mailto:xlxd-star@yahoogroups.com>> wrote:
>>
>> Hi Yngwie,
>>
>>
>> I have a USB-3012 which is recognized as 4, 3-channel devices. So 12
>> channels are seen.
>>
>> Bob/W6KD pointed out that the ThumbDV uses the FTDI FT230XS
>> serial-to-USB chip. The DVSI units use the FT232R, but both use the
>> same unified driver set. Apparently FTDI has a Facebook page and
>> describes the differences.
>>
>> Might be useful to look there and also on the FTDI site and see if any
>> differences might indicate different settings in the drivers. Just a
>> thought.
>>
>> Good luck!
>>
>> John
>> K6KD
>>
>
