Hi guys,

First of all, the dashboard has nothing to do with the interlinks.
Interlinks are controlled by the xlxd service depending on your xlxd.interlink file and your black and white lists.

If you have problems with your interlinks, the first thing to do is to read the doc about interlinks and to understand how the interlink works.

Double check the xlxd.interlink on both xlx servers.
Comment the not working interlink out in your xlxd.interlink, wait until the gatekeeper reloads the xlxd.interlink and try again. (both sides).
Better use the dns name of your peers instead the IP.
A lot of XLX sysops have no fix IP and are using dyndns.

Best practice to run an XLX server with interlinks :

- run your server on a server environment, raspi is not recommended.
- take care to have a fix IP and a stable internet connection, dsl or mobile lines are not recommended.
- stay in touch with your peers sysops to coordinate your configuration.

For testing or playing around with an XLX server, a Pi behind a privat DSL line will do the job.
But at the moment you really like to run a public XLX with real load, you should respect the best practices.
It is more than frustrated for the users if they have drop outs or  disconnects all the time because the server cannot handle the load.

73,  Luc
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まず第一に、ダッシュボードはインターリンクとは関係がありません。
インターリンクは、xlxd.interlinkファイルと黒と白のリストに応じて、xlxdサービスによって制御されます。

インターリンクに問題がある場合は、最初に行うべきことは、インターリンクに関する文書を読み、インタリンクの仕組みを理解することです。

両方のxlxサーバーでxlxd.interlinkをダブルチェックします。
あなたのxlxd.interlinkで動作していないインターリンクをコメントアウトし、ゲートキーパーがxlxd.interlinkを再ロードしてやり直すまで待ってください。 （両側）。
IPの代わりにピアのDNS名を使用する方が良い。
XLXのsysopsの多くは、修正されたIPを持たず、dyndnsを使用しています。

インターリンクを使用してXLXサーバーを実行するためのベストプラクティス：

- サーバー環境でサーバーを実行すると、raspiは推奨されません。
- 固定IPと安定したインターネット接続があるように注意してください.DSLまたはモバイル回線はお勧めしません。
- あなたの構成を調整するためにあなたの同僚のsysopsと連絡を取る。

テストやXLXサーバーでの再生のために、privat DSLラインの後ろにあるPiがその仕事をします。
しかし、現実の負荷でパブリックなXLXを実行したいと思う瞬間、ベストプラクティスを尊重する必要があります。
サーバーが負荷を処理できないため、ユーザーがいつでも中断または切断した場合、ユーザーにとっては不満が増します。
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