It has been my experience that if you only have (1) entry in your interlink file, a second blank line is needed.
Again, this has been my experience. I have XLX026 which has several entries and it works great. I couldn't get 026 to interlink to 603. Once I added a blank second line to the interlink file on 603, they connected and have been working together very nicely.

The XLX reflector software is absolutely the best we have used and to Luc and team, thank you for providing this software and support!

Mark, W1DDI.

私の経験では、インターリンクファイルに（1）エントリしかない場合、2番目の空行が必要です。
これも私の経験でした。 私はいくつかのエントリを持ってXLX026を持って、それは素晴らしい作品です。 私は026を603に連動させることができませんでした.603のインターリンクファイルに空白の2行目を追加すると、彼らは接続し、とてもうまく一緒に作業していました。

XLXリフレクターソフトウェアは、私たちが使用しているLucとチームにとって最高のものです。このソフトウェアとサポートを提供してくれてありがとう！

マーク、W1DDI。













Did you read the doc about interlink connections located in the file section ?

Interlinks are only possible from XLX to XLX, not from XLX to XRF.
So if you like to interlink XLX011 to XLX093 on module B you need one entry in the xlxd.interlink on each side.

for XLX011 the xlxd.interlink should be:

XLX093 xrf093.kb8pmy.net B

on XLX093 the xlxd.interlink should be:

XLX011 xlx011.warn.org B

Let me know if it works.
73, Luc

ファイルセクションにあるインターリンク接続についての文書を読んだことがありますか？
XLXからXLXへのインターリンクのみ可能で、XLXからXRFへのインターリンクは不可能です。
したがって、モジュールBのXLX011とXLX093を相互リンクする場合は、各側のxlxd.interlinkに1つのエントリが必要です。
XLX011の場合、xlxd.interlinkは次のようになります。
XLX093 xrf093.kb8pmy.net B
XLX093では、xlxd.interlinkは次のようになります。
XLX011 xlx011.warn.org B
それが動作するかどうか私に教えてください。
73、リュック
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Here are the four related ongoing entries in my log...

: Sending connect packet to XLX peer XRF093   @ 98.29.xx.xxx for modules B
(my server is trying to connect to your module B)

: XLX ack packet for modules B from XLX093   at 98.29.xx.xxx
(I'm receiving something back from your server - a rejection is usually "nack" and not "ack", so I'm not sure exactly what this means)

: XLX (1.4.2) connect packet for modules B from XLX093   at 98.29.xx.xxx
(I'm receiving the connect request from your server)

: Gatekeeper blocking linking of XLX093   @ 98.29.xx.xxx using protocol 4
(I'm rejecting your request, which I think would mean my xlxd.interlink file doesn't see anything that matches the request)

This is the same in both our logs. I am not sure what is wrong.

Started with xlxd and local ipaddress

interlink file is xlx011 xlx011.warn.org B 

Still getting errors

Thanks,

Ryan (KB8PMY)
KD8TUZ Hamilton Wireless Radio Club

ここに私のログに4つの関連する進行中のエントリがあります...

：モジュールBのXLXピアXRF093 @ 98.29.xx.xxxへの接続パケットの送信
（私のサーバがあなたのモジュールBに接続しようとしています）

：98.29.xx.xxxのXLX093のモジュールBのXLX ackパケット
（私はあなたのサーバから何かを受け取っています - 拒絶は通常 "ナック"であり、 "ack"ではないので、これが何を意味するのか正確にはわかりません）

：XLX（1.4.2）はモジュールBのパケットをXLX093から98.29.xx.xxxに接続します
（私はあなたのサーバーからの接続要求を受け取ります）

：プロトコル4を使用しているXLX093 @ 98.29.xx.xxxのゲートキーパーブロッキングリンク
（私はxlxd.interlinkファイルに要求と一致するものが何も表示されないというあなたの要求を拒否しています）

これは両方のログで同じです。 何が間違っているのか分かりません。

xlxdとローカルipaddressで始まる

インターリンクファイルはxlx011 xlx011.warn.org Bです

まだエラーが発生しています

ありがとう、

ライアン（KB8PMY）
KD8TUZハミルトンワイヤレスラジオクラブ
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