Hello Luc,

First of all thank you for the good work on XLX reflector. I stil need to update and wil do that next week.

What i noticed with the new dashboard v2.3.4. you need to fill in and apply the filter within the reload timer of the html page. Just a tip to use javascript to refresh in a future version so that only data is refreshed. Don't know if this is possible?

And can you explain what the new active loop detection exactly does do. Since we have some issues sometimes with the interlinks in the Netherlands (Accidental broken conversation... next conversation is ok again) and were not sure if it are the interlinks or the connection to the clients... Could it be that this is for solving this issue?

Kind regards and 73's.

PH0DV
Dick
 ハロー・リック、

まずXLXリフレクターの良い仕事に感謝します。 私は更新する必要があり、来週にそれを行う必要があります。

私は新しいダッシュボードv2.3.4に気づいた。 htmlページのリロードタイマーでフィルタを入力して適用する必要があります。 将来のバージョンで更新するためにjavascriptを使用して、データのみを更新するヒント。 これが可能かどうか分かりませんか？

新しいアクティブループ検出が正確に何をするのか説明できますか？ 私たちはオランダのインターリンクで時々問題を抱えています（偶然の壊れた会話...次の会話はもう一度大丈夫です）、それがインターリンクかクライアントへの接続かどうかはわかりませんでした。 この問題を解決するには？

親切な意見と73's。
__._,_.___

Hi Dick,

The refresh is by design. If you feel that 10 seconds are not enough to use the filter, you can increase the refresh time in the config.inc.php.
I hate java and java script, so this is no option for me, but the source is open, so feel free to add a fork with java implementation J

Here the working principle of the xlx loop detection.

When opening a new incoming stream, the system checks that the streamid of this new stream is unique, that is not equal to the streamid of another stream in progress.
If the streamid is unique, and the origin is allowed by the gatekeeper, then the system opens the stream and registers the original IP.
Next, for all subsequent incoming packets (ie DV frames), the system verifies that the original IP corresponds to the one registered for that streamid. 
It therefore ignores all the packets whose original IP does not correspond to that which was recorded for at the opening of the stream.

This is completely transparent to the user.

73, Luc

こんにちはディック、

リフレッシュは設計によるものです。 フィルタを使用するには10秒で十分でないと感じる場合は、config.inc.phpでリフレッシュ時間を長くすることができます。
私はjavaとjavaスクリプトが嫌いですので、これは私のためのオプションではありませんが、ソースはオープンなので、java実装のJ

ここでxlxループ検出の動作原理。

新しい着信ストリームを開くとき、システムはこの新しいストリームのstreamidが一意であることを確認します。これは進行中の別のストリームのstreamidと等しくありません。
streamidが一意で、ゲートキーパーによって原点が許可されている場合、システムはストリームを開き、元のIPを登録します。
次に、後続のすべての着信パケット（すなわちDVフレーム）について、システムは元のIPがそのストリームIDに登録されたIPに対応することを確認する。
したがって、元のIPがストリームの開始時に記録されたIPに対応しないパケットはすべて無視されます。

これは、ユーザーにとっては完全に透過的です。
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