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QST QST QST
Parachute Mobile Mission 26 is set for May 13, 2017.
Make a contact with a skydiver and receive a one-of-a-kind QSL card.
WHERE: We will be conducting our Mission from Bay Area Skydiving, Byron Airport, Byron, CA.


先ず、お互いの国の背景を考慮する必要があると思いますが、私の考えは５６９と５９５を区別して使いたいのです。

海外でのリフレクターの使われ方はよく知りませんが５６９を含む日本国内のXLXリフレクターはAモードのリンクもありますがBモードでリンクされた日本語のQSOが主体です。

私の認識は海外のD－StarのソフトはG2とかG3ですが日本ではいまだにG1のためREFリフレクターは使えませんので日本のリフレクターシステムは非常に遅れています。

私は５９５のリンクをモードAに限定して海外局とのQSOを主体にしたいのです。
HF帯のコンディションが低調になっていくこれからはこのようなリフレクターをD-Starの初心者にHF帯を使うことなく海外局とのQSOができる有効な手段であることを伝えたいのです。

勿論国内にはD-Starのリピーターがありこれを通して海外局にアクセスしても応答はリフレクターからしかないのが現状です。
REFリフレクターに代ってXLXリフレクターが普及することを望んでいます。






[bookmark: _GoBack]Hello John,

Please excuse me to comment on long sentences here.
First of all, I think that it is necessary to consider the background of each other's countries, but my opinion wants to distinguish between 569 and 595.
Although I do not know well how to use reflectors in abroad, XLX reflectors in Japan including 569 have links for A mode but mainly Japanese language QSO in B mode.
My perception is that overseas D - Star software is G2 or G3 but in Japan it is still G1 so we are not able to use the REF reflector so Japan's reflector system is very behind of you.
I would like to focus on QSO with overseas stations by limiting the link of 595 to mode A.
Since the propagation condition of the HF band will become sluggish from now on,  I want to tell the lovers of D-Star (especially novice) that such a reflector is an effective means to do QSO with overseas stations without using the HF band.
Of course, there are repeaters of D - Star domestically, and even if you use this to access overseas stations, there is currently only response from the reflector.
So most people have not responded from repeater so they are giving up QSO with overseas stations I hope the XLX reflector will become popular instead of the REF reflector.. 

Please accept my wish.

Best Regards,
Shu JA3GQJ
